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[~ Mulicast IP Address
 Obtain P address fom DHCP

" Use addresses fom the follwing range:

1Pv4 From: [79001 To: [7R00254

IPG From: [FF15:1 To: [FFI5:FF

Note: Ve that there i o overlap between tis range and [P
adkresses being used by other mulicastservers on your netvirk.

More information about these selfinas

[~ Transfer Setings
 Keep allmulicast cliets in a session at the same speed
 Separate clients in thie sessions (slow, medium, fast]

 Separate clients inta to sessions (sow and fast).

 Automatical dsconnect clients below this speed (in KBps) [757

Cone |y

fact that the client can't read the boot configuration data seems to
point to this conclusion. I haven't verified it as a fix yet, T will
be working with the networking techs on this very soon.

Dan Van Drunen Re: PXE Problems booting to WDS Server
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