How to slipstream Intel SATA (ICH7M) driver with XP


1. Extract Intel SATA drivers (10.1_f6flpy-x86.zip) with 7-Zip(free) or WinRar.
2. Get your Windows XP installation disc and copy the contents to a new folder on HDD.
3. Run nLite, select your language and choose ‘ Next ‘.
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4. Click on ‘ Browse… ‘ and point folder with copied XP files. Mine was in E:\WinXP.
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Now you should check with which Service Pack (SP) is your XP disc. It should be at least SP2 like in below example. If it’s lower, then in point 6 you will find out how to deal with this problem.

[image: image3.png]nlite

e

Product name: Windows XP Professional
Language: Polish

Service Pack: 2

Version: 5126002180

Path: EXWIRKP.

Size: 43047MB

@ (=)

Ty





5. Choose ‘ Next ‘.
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6. When your installation disc is with SP0 or SP1 then (otherwise skip to point 7):

Download SP2 from Microsoft site (set your XP language there). In ‘ Task Selection ‘ choose ‘ Service Pack ‘,  ‘ Drivers ‘ and ‘ Bootable ISO ’. Click ‘ Next ‘.
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Choose ‘ Select ‘
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and point SP2 file.
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nLite will automatically extract and integrate it with your windows files folder.
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SP2 is slipstreamed now. Choose ‘ Next ‘ and skip to point 8.
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7.  When your installation disc is with SP2 or SP3, then in ‘ Task Selection ‘ choose 

      ‘ Drivers ‘ and ‘ Bootable ISO ’and click on ‘ Next ‘.
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8. Choose ‘ Insert ‘
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and click on ‘ Single driver ‘.
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9. Go to folder with extracted Intel SATA drivers from point 1 and click twice with left button of your mouse on iaAHCI file.
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10. In this step choose ‘ Textmode driver ‘ and  select ‘ ICH7M/MDH SATA AHCI Controller ‘
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11. Click on ‘ Next ‘.
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12. Choose here ‘ Yes ‘. This will start slipstreaming SATA drivers process to folder with XP.
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13. You will see now progressive stripes.
[image: image17.png]nlite =

Freparing selected tasks

Integrating hotfixes, packs and themes

Rermnoving cormponents

Processing setup files

Integrating drivers

Finalizing

Normal -

&y @os | o




14. When nLite will finish this task you will be informed about it like on below photo.
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15. In this final step you may:

● create ISO image to burn it later 

● burn new XP copy directly on CD-R disc.
Option 1. Creating ISO image:
Before you will do anything you may want to change standard ‘ Label ‘ name for something else. Under ‘ Mode ’ choose ’ Create Image ‘,  and click on ‘ Make ISO ‘ button. After this action you will have to choose where you want to save iso file and how it should be named.
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In lower part of this window will show up information then this process ended with success.
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When you will want to burn this iso, then run again nLite and in ‘ Task Selection ‘ choose only ‘ Bootable ISO ’. Click on ‘ Next ‘. This time under ‘ Mode ’ select ’ Burn Image ‘ and choose ‘ Burn ‘. Find location of your iso file and click twice on it.
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Option 2. Directly burning new XP CD/DVD:
Before you will do anything you may want to change standard ‘ Label ‘ name for something else. Under ‘ Mode ’ choose ‘ Direct Burn ‘ and click on ‘ Burn ‘ button.
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Choose ‘ Yes ‘ to burn it to CD-R. Wait for it to finish.
[image: image23.png]Bootable IS0

Goner
ode Devie
(R00F.HLOT ST GVORAM G621 Hadh

Direet Bun

Label Bur speed Meda
WirkP

Advanced

150 Engine
@ Burm the content to the mediia?
Defat

] Quick erase.

7] Test wite

Progress

=3 |

Infarmation
1fyou want o nclude additonal fles an your CD/DVD, capy them ta the warking diectory

(B G0n ey
—
@ o)





16. Choose ‘ Next ‘and click on ‘ Finish ‘ to exit nLite.
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