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[Note] Asterisks(*) indicate that parameters obtained from DHCP server will take priority over the entry fields when DHCP is set to Active.
Values in parentheses( ) indicate current operating parameters.

B 1Pv4 : Active

Ethernet
 Host Name. : RNPF1DA82
u DHCP Active © Inactive
B Domain Name + © Auto-Obtain (DHCP)
Specify
dbwie.local
 1Pv4 Address = ©192.168.0.254 (192.168.0.254)
® Subnet Mask = : [255.255.255.0 (255.255.255.0)
= DDNS M
= WINS
W Primary WINS Server = (0.0.0.0)
W Secondary WINS Server = (0.0.0.0)
™ Scope ID = : 0
Details A
 Default Gateway Address = : |192.168.0.1 (192.168.0.1)
H DNS Server © | Auto-Obtain (DHCP) © Specify.
Auto-Obtain (DHCP)
DNS Server1(DHCP) .0.0.0
DNS Server2(DHCP)  0.0.0 -
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® Primary WINS Server = :
W Secondary WINS Server = :

 Scope ID = 3

Details
W Default Gateway Address =
H DNS Server

Auto-Obtain (DHCP)

DNS Server1(DHCP)
DNS Server2(DHCP)

DNS Servera
Specify

DNS Server1
DNS Server2

DNS Server3
n LR

W RSH/RCP

= DIPRINT

nFP

= sftp

W WSD (Device)

® WSD (Printer)

B WSD (Scanner)

npp

W WSD (Printer)/IPP Timeout
mRpp

[) WinScribeNET [ Ricoh 4000-Web1m... [ Ricoh 5000-Weblm... 3 Culpeper Chamber...

0.0.0.0 (0.0.0.0)
0.0.0.0 (0.0.0.0)
0

:192.168.0.1 (192.168.0.1)
© | Auto-Obtain (DHCP) © Specify.

.0.0.0

.0.0.0
: [192.168.0.102 ‘The parameter setting will be updated only when [Auto-Obtain (DHCP)] is clicked.
: [192.168.0.102 The parameter setting will be updated only when [Specify] is clicked.
:[192.168.0.103
:10.0.0.0
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