NON-CONVERGED TOPOLOGY (DCB PFC/ETS)                                        OS10, 10Gbe/100Gbe
QLOGICTCP RDMA	QUICK-START WSSD
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	 S4112F-ON (TOR1)
	 S4112F-ON (TOR2)

	
Configure terminal 
hostname S4112F-TOR1
!
 interface mgmt1/1/1
 no shutdown
 no ip address dhcp
 ip address 192.168.255.1/30
 ipv6 address autoconfig
!
interface range ethernet1/1/11-1/1/12
 description VLTiLink
 no shutdown
 no switchport
!
interface port-channel10
 description CORE.UPLINK
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 interface vlan 200
 exit
 interface port-channel10
 switchport trunk allowed vlan 200
 vlt-port-channel 10
! 
interface range ethernet1/1/7-1/1/10
 description CORE.UPLINK
 no shutdown
 channel-group 10 mode active
 no switchport
 flowcontrol receive on
 flowcontrol transmit off
!
vlt-domain 1
 backup destination 192.168.255.2
 discovery-interface ethernet1/1/11
 discovery-interface ethernet1/1/12
 vlt-mac 00:00:00:00:00:02
!
interface range ethernet1/1/1-1/1/4
 description MGMT.PORTS
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 switchport trunk allowed vlan 200
 flowcontrol receive on
 flowcontrol transmit off
 spanning-tree disable
 spanning-tree port type edge
!
interface range ethernet1/1/13-1/1/14
 description STOR.PORTS
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 interface vlan 301
 interface vlan 302
 exit
 interface range ethernet1/1/13-1/1/14
 switchport trunk allowed vlan 301,302
 mtu 9216
 flowcontrol receive on
 flowcontrol transmit off
 spanning-tree disable
 spanning-tree port type edge
!
interface Vlan 200
 description MANAGEMENT
 no shutdown
 ip address 172.18.100.124/25
 vrrp-group 200
 virtual-address 172.18.100.126
! 
interface Vlan 301
 description STORAGE-1
 no ip address
 mtu 9216
 no shutdown
! 
interface Vlan 302
 description STORAGE-2
 no ip address
 mtu 9216
 no shutdown
! 
lldp enable
!
ip ssh server enable
!
write memory

	
Configure terminal
hostname S4112F-TOR2
!
interface mgmt1/1/1
 no shutdown
 no ip address dhcp
 ip address 192.168.255.2/30
 ipv6 address autoconfig
!
interface range ethernet1/1/11-1/1/12
 description VLTiLink
 no shutdown
 no switchport
!
interface port-channel10
 description CORE.UPLINK
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 interface vlan 200
 exit
 interface port-channel10
 switchport trunk allowed vlan 200
 vlt-port-channel 10
! 
interface range ethernet1/1/7-1/1/10
 description CORE.UPLINK
 no shutdown
 channel-group 10 mode active
 no switchport
 flowcontrol receive on
 flowcontrol transmit off
!
vlt-domain 1
 backup destination 192.168.255.1
 discovery-interface ethernet1/1/11
 discovery-interface ethernet1/1/12
 vlt-mac 00:00:00:00:00:02
!
interface range ethernet1/1/1-1/1/4
 description MGMT.PORTS
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 switchport trunk allowed vlan 200
 flowcontrol receive on
 flowcontrol transmit off
 spanning-tree disable
 spanning-tree port type edge
!
interface range ethernet1/1/13-1/1/14
 description STOR.PORTS
 no shutdown
 switchport mode trunk
 switchport access vlan 1
 interface vlan 301
 interface vlan 302
 exit
 interface range ethernet1/1/13-1/1/14
 switchport trunk allowed vlan 301,302
 mtu 9216
 flowcontrol receive on
 flowcontrol transmit off
 spanning-tree disable
 spanning-tree port type edge
!
interface Vlan 200
 description MANAGEMENT
 no shutdown
 ip address 172.18.100.125/25
 vrrp-group 200
 virtual-address 172.18.100.126
! 
interface Vlan 301
 description STORAGE-1
 no ip address
 mtu 9216
 no shutdown
! 
interface Vlan 302
 description STORAGE-2
 no ip address
 mtu 9216
 no shutdown
! 
lldp enable
!
ip ssh server enable
!
write memory 
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