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The USB Board requires no settings.
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What's New?

1. Dual device support
Allows you to attach an RF hub to enable Voting and Slate devices on a non
RF board.

2. Microsoft Signed Driver
No user intervention needed when the user connects usb or serial devices.

3. Can be deployed by MSI

Unlike Activdriver 2 or 3, Activdriver 4 comes as a standard msi and is
deployable from a 2003 or RM server.

4. Dual Display Compliant

This means you can have the board as an extended desktop of your computer,

orly where setup is montor 1 - 2andnot2- 1

5. 64bit capable

Can be used with 64 bit versions of XP and future vista.

6. Can be used with com ports higher than 8

With the previous driver it was restricted to com ports 1-8, the driver will now
support all com ports on the system and will only list the ones available.
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Changes
AV icon has changed.
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As you can see if you hover over the flame icon you see how many devices have F

been detected.
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Changes
The About box is different.
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As you can see the new about tab gives you more information, plus the 0
actual driver version F
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Changes

The Settings box is different.
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As you can see the new settings tab gives more options including a

double click speed optf

ion.
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Changes

There are more options in the calibration of the activboard / slate.

When you have a board connected to a pc with extended desktop, you )

are asked which monitor you want to calibrate the board with.
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Select the screen you want to calbrate.
Do you want to calbrate sereer 17
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This only works when you have the monitor 1 on the left and monitor 2
on the right.
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Changes

There are more options in the calibration of the activboard / slate.

When you have a hub and slate connected to a pc with extended
desktop, you are asked which monitor you want to use the slate with.

You are cannectzd to a hub.
Do you wart to calbrate the system for use with a slate 7

i S

Select the screen you want to calbrate.
~ Do you want to calbrate sereer 17
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This only works when you have the monitor 1 on the left and monitor 2 o
on the right.




