Conecting to your VPN

Assuming you have windows XP and an 'always on' internet connection...

Right click on My Network places and select properties to bring up your existing network connections. Click on create new connection under the Network Tasks list. 
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Follow the screen shots below filling in the relevant details.
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::::: ms-ras.cleo.net.uk below :::::
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Click finish. You should now see a new connection 'Norden' as below.
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Double click on the connection and enter your usual user name with its full domain name (EG – user@school.region.sch.uk) and your usual network password. If this connects successfully you should now be able to access network resources. We use Remote Desktop, some protocols are filtered by Cleo so you may have to do a bit of trial and error.

Hope this helps!

